- Top
- Shooting
- Setting of time data
- Setting user bits

# Setting user bits

Set the user bits to be recorded.

Select the user bits to record in the [RECORDING] menu → [TC/UB] → [UB MODE].

[FRAME RATE] | Selects the image information (such as frame rate) of the camera.
[USER] | Selects the set user bits.
[TIME] | Selects the local time. (hh, mm, ss)
[DATE] | Selects the local date and time. (YY, MM, DD, hh)
[TC] | Records the time code value as user bits.
[CLIP NAME] | Records the value that CAM INDEX (one character) and CARD COUNT (three-digit number) are converted to ASCII character code. Only enabled when the [SYSTEM] menu → [FILE FORMAT] → [MOV] is set.

## Memory function of the user bits

Setting contents of the user bits is automatically recorded, and it is maintained even if the power is set to < > (standby).

Top of the page