- Top
- Shooting
- Basic procedures
- Preparation

# Preparation

Attach the fully charged battery, or connect the AC adaptor. (Power supply)

Set the power switch to <ON>. (Turning on/off the power)

Insert the P2 card. (Inserting a P2 card)

Adjust the angle of the LCD monitor and viewfinder or other conditions. (Using the LCD monitor, Using the viewfinder)

Set the lens cover lever to <OPEN>. (Opening and closing the lens cover)

NOTE

- Even if the battery is fully charged, the remaining capacity of the battery may not be correctly displayed.

Top of the page