- Top
- Shooting
- Streaming function
- List of system modes and supported streaming output

# List of system modes and supported streaming output

The following shows the relationship between system modes and streaming modes on this camera.

- “✓” are supported, and “—” are not supported.

[SYSTEM MODE] | [STREAMING MODE]
--- | ---
[LINE&FREQ] | [REC FORMAT] | HD streaming [AVC-G6], [AVC-G (QoS)] | SD streaming [HQ], [LOW], [SHQ (QoS)]
[1080-59.94i] | [AVC-I100/60i] | ✓ | ✓
[AVC-I50/60i] | — | ✓
[AVC-G50/60i] | ✓ | ✓
[AVC-G25/60i] | ✓ | ✓
[1080-50i] | [AVC-I100/50i] | ✓ | ✓
[AVC-I50/50i] | — | ✓
[AVC-G50/50i] | ✓ | ✓
[AVC-G25/50i] | ✓ | ✓
[720-59.94P] | [AVC-I100/60P] | ✓ | ✓*
[AVC-I50/60P] | — | ✓*
[AVC-G50/60P] | ✓ | ✓*
[AVC-G25/60P] | ✓ | ✓*
[720-50P] | [AVC-I100/50P] | ✓ | ✓*
[AVC-I50/50P] | — | ✓*
[AVC-G50/50P] | ✓ | ✓*
[AVC-G25/50P] | ✓ | ✓*

[LOW] cannot be selected.

Top of the page