- Top
- Shooting
- Special recording functions
- One-shot recording

# One-shot recording

Recording takes place once for the set amount of time.

Set all items in the main menu → [SYSTEM MODE].

Select [ONE SHOT] in the main menu → [RECORDING SETUP] → [RECORDING].

Set the time with [ONE SHOT TIME] in the main menu → [RECORDING SETUP] → [RECORDING SETTING].

Press the REC button.

- Once recording has taken place for the set amount of time, recording will pause.

- To stop recording, press the <> button.

- To clear settings, set [NORMAL] in the main menu → [RECORDING SETUP] → [RECORDING].

- When [OFF] is set in the main menu → [RECORDING SETUP] → [RECORDING SETTING] → [RECORDING HOLD], one-shot recording settings are cleared by turning off the camera.

- [I-REC] is displayed while recording, and [I-] is displayed while paused.

- When recording is stopped, [I-] flashes.

NOTE

- While in operation, other operations are unavailable.

- Pre-recording and one-clip recording will not operate.

- Audio is not recorded.

- Recorded data (data recorded until the camera was stopped) is included in one file.

- When one-shot recording is continuously performed, the recording operation may be slower.

Top of the page