- Top
- Preparation
- Attaching and adjusting accessories
- Attaching a tripod

# Attaching a tripod

The tripod attachment holes accept 1/4-20 UNC and 3/8-16 UNC screws. Use the hole that matches the diameter of the clamping screw on the tripod.

NOTE

- Use a tripod in safe locations.

- The depth of the tripod attachment hole is 5.5 mm. When attaching the camera to a tripod, do not over-tighten the tripod screw.

Top of the page