- Top
- Shooting
- Handling setting data
- Saving to an SD memory card and loading saved data

# Saving to an SD memory card and loading saved data

Scene files and other setting values that you have set can be saved as a file, and up to 8 files can be saved on the SD memory card, and saved data can be loaded.

- For scene files, the current setting values are saved in the camera automatically, and you can write the saved data to an SD memory card. When they are loaded from the SD memory card, the current setting values are overwritten as well as the data saved in the camera.

- All scene files [F1:] to [F6:] are overwritten.

## Saving scene files

Fig. 1

Fig. 2

Select [SAVE] in the main menu → [CARD FUNCTIONS] → [SCENE FILE]. (Fig. 1)

Select a file number (1 to 8) and press the control stick (or <SEL/PUSH SET> dial button). (Fig. 2)

The title entry screen and keyboard are displayed.

Enter desired characters on the keyboard using the control stick (or <SEL/PUSH SET> dial button).

Select [OK] on the keyboard and press the control stick (or <SEL/PUSH SET> dial button).

A confirmation screen is displayed.

Select [YES] and press the control stick (or <SEL/PUSH SET> dial button).

The file is written with the entered title on the SD memory card, and the screen of Fig. 2 returns.

## Loading scene files

Select [LOAD] in the main menu → [CARD FUNCTIONS] → [SCENE FILE].

Select a file number (1 - 8) and press the control stick (or <SEL/PUSH SET> dial button).

A confirmation screen is displayed.

Select [YES] and press the control stick (or <SEL/PUSH SET> dial button).

When loading is completed, [LOAD OK] is displayed.

## Saving and loading user files

Select [SAVE] or [LOAD] in the main menu → [CARD FUNCTIONS] → [USER FILE]. The operations onward are the same as for scene files.

Top of the page