- Top
- Shooting
- Adjusting image quality
- Knee function

# Knee function

This function sets the compression of video signals to prevent halation in images.

#### General settings

Use the camera with the factory settings.

#### Advanced settings

Configure the settings in the main menu → [SCENE FILE] → [KNEE SETTING].

[KNEE MODE]: Sets the operation mode of knee function ([AUTO]/[MANUAL]/[OFF]).

- When [AUTO] is selected in [KNEE SETTING]

  [A.KNEE RESPONSE]: Sets the speed of response. Smaller values make the response faster.

- When [MANUAL] is selected in [KNEE SETTING]

  [KNEE MASTER POINT]: Sets the knee point position in 0.5% steps.

  [KNEE MASTER SLOPE]: Sets the knee inclination.

  [KNEE MASTER SLOPE Rch]: Sets the knee inclination of Rch.

  [KNEE MASTER SLOPE Bch]: Sets the knee inclination of Bch.

Top of the page