- Top
- Shooting
- Special recording functions
- Interval recording

# Interval recording

The camera will record one frame at each set time interval.

1 frame recording

1 frame recording

1 frame recording

(Time)

[INTERVAL TIME] set time

[INTERVAL TIME] set time

Set all items in the main menu → [SYSTEM MODE].

Set [INTERVAL] in the main menu → [RECORDING SETUP] → [RECORDING].

Set the time in the main menu → [RECORDING SETUP] → [RECORDING SETTING] → [INTERVAL TIME].

Press the REC button.

- The camera will repeat the operation of one frame recording at each set time interval.

- To stop recording, press the <> button.

- To clear settings, set [NORMAL] in the main menu → [RECORDING SETUP] → [RECORDING].

- When [OFF] is set in the main menu → [RECORDING SETUP] → [RECORDING SETTING] → [RECORDING HOLD], interval recording settings are cleared by turning off the camera.

- [I-REC] is displayed while recording, and [I-] is displayed while paused. However, if the setting in step 3 is less than two seconds, [I-REC] flashes according to the set interval time.

- When recording is stopped, [I-] flashes.

NOTE

- Pre-recording and one-clip recording will not operate.

- Audio is not recorded.

- Recorded data (data recorded until the camera was stopped) is included in one file.

Top of the page