- Top
- Preparation
- Attaching and adjusting accessories
- Attaching the front microphone

# Attaching the front microphone

Microphones such as a super-directional microphone AG-MC200G (optional) can be attached.

Screws for tapped hole protection are attached on the camera body. Remove those screws when you attach the microphone holder.

Screw for the microphone holder

Microphone cable clamp

Microphone holder

<AUDIO INPUT 1> terminal

Fig. 1

Fig. 2

Fig. 3

Attach the microphone holder. (Fig. 1)

Attach the microphone and tighten the microphone holder clamping screw. (Fig. 2)

Connect the microphone connecting cable to the <AUDIO INPUT 1> terminal on the camera. (Fig. 3)

Secure the microphone connecting cable with the microphone cable clamp.

Set the <INPUT 1> switch to match the microphone to be connected.

NOTE

- The microphone holder cannot be fixed with the screws originally attached on the camera. Use the dedicated screws that came with the camera to fix the microphone holder.

Top of the page