- Top
- Overview
- What you can do with this camera
- Linking to external devices

# Linking to external devices

## USB device mode

Data (files) for performing nonlinear editing on a computer are transferred.

P2 memory card, microP2 memory card*1

USB 2.0 (device mode)*2

Personal computer

P2 memory cards and microP2 memory cards are optionally available. They are not supplied with the camera.

The USB 2.0 cable is not supplied with the camera. Prepare a commercial USB 2.0 cable (double-shielded for noise suppression).

## USB host mode (<USB3.0 HOST> terminal connection)

The camera directly controls the hard disk drive to transfer data.

USB 3.0*

External storage device

A USB 3.0 cable is not supplied with this product. Use a commercially sold USB 3.0 cable (with double shielding for noise reduction).

## Connecting to the remote operation panel (AK-HRP200G)

You can remote control some functions by connecting the remote operation panel AK-HRP200G (optional) using a LAN cable.

AK-HRP200G

LAN

## Connecting to monitor

A monitor can be connected to output images.

Audio pin cable*1

Monitor

HDMI cable*2

BNC cable (composite/HD SDI/SD SDI)*3

Cables are optionally available. They are not supplied with the camera.

Use an HDMI cable (optional) with double shielding. For the HDMI cable, using Panasonic HDMI cable is recommended.

For the BNC cable (optional) connected to the <SDI OUT> terminal, prepare a double-shielded cable equivalent to 5C-FB.

Top of the page