- Top
- Playback
- Thumbnail operations
- Restoring clips

# Restoring clips

You can restore clips that were made defective as a result of sudden power-down during recording or removal of the P2 card being accessed.

Use the control stick to move the cursor over the clip to be restored (defective clips are indicated by defective clip marks) and press the control stick to select the clip.

Select [REPAIR] in the main menu → [CLIP] and press the control stick.

Select [YES] using the control stick.

This restores the clip.

NOTE

- To find defective clips, set the main menu → [CLIP] → [REPOSITION] to [NG CLIPS]. Only defective clips are displayed. For details, refer to “Setting thumbnails to be displayed”.

- You can restore clips with yellow defective clip indicators. Delete clips with red defective clip indicators. If the clips cannot be deleted, format the P2 card.

  During restoration of the clips, however, the defective clip indicator may change from yellow to red, and result in the inability to restore the clips.

- When defective clips containing proxy data are restored, proxy data will be deleted.

Top of the page