- Top
- Overview
- What you can do with this camera

# What you can do with this camera

This camera is a P2 hand-held camera recorder with the following features.

- The camera has an optical 22x cam-type zoom and a newly-developed 1/3-type 2.2 million pixel 3MOS sensor with high sensitivity F11 (59.94 Hz)/F12 (50 Hz) and low noise.

- In addition to AVC-Intra 200/AVC-Intra 100/AVC-Intra 50, as a recording codec, the camera also has a low-rate and full HD (1920×1080, 4:2:2, 10-bit) image quality AVC-LongG 50/AVC-LongG 25, and is also capable of long time recording with AVC-LongG 12 (4:2:0, 8-bit).

- It is compatible with both microP2 memory cards and P2 memory cards.

- It supports progressive full frame rate shooting in 1080/60P, 1080/50P, 720/60P, and 720/50P, output of 3G SDI/HDMI, and operations using AVC proxy video.

- In addition to metadata input and playlist editing by using both wired and wireless LAN connections, you can send proxy files to the network server by connecting 4G/LTE USB modem (optional).

  Also, high speed network connection is possible by connecting an external bonding device.

  For details on bonding device that can be connected, visit the support desk at the following website:

  https://pro-av.panasonic.net/

- Video streaming transmission is supported. You can distribute live stream while recording video in a memory card.

Recording to the memory card
Linking to external devices
Connecting to the network
Top of the page