- Top
- Connecting to External Devices
- Connecting to the remote operation panel (AK-HRP200G)
- Switch function in remote control mode

# Switch function in remote control mode

The following switches and buttons on the camera do not function in remote control mode.

- <MENU> button

- <SEL/PUSH SET> dial button

- <GAIN> switch

- <WHITE BAL> switch (works when set in the <A> position)

- <BARS> button

- Manual focus operation using the focus ring

- Switching between auto focus mode and manual focus mode using the <FOCUS> switch

- Motorized zoom operation of the zoom lever (grip side/handle side)

Top of the page