- Top
- Preparation
- Power supply
- Using the AC adaptor

# Using the AC adaptor

## Attaching

To the power outlet

<DC IN 12V> terminal

Connect an AC cable.

Connect in the order shown in the figure.

Connect the AC adaptor to the <DC IN 12V> terminal.

## Removing

Turn the power switch to <OFF> while holding down the lock release button.

Make sure that the LCD monitor has gone off.

Remove the AC adaptor from the <DC IN 12V> terminal.

NOTE

- When not using the camera, remove the AC cable from the power outlet.

- Use the supplied AC adaptor. Do not use other AC adaptors.

- The AC adaptor can be connected when attaching the battery to the camera. When the AC adaptor is connected, the camera will switch to be powered by the AC adaptor. When removing the AC adaptor, the camera will be powered by the battery.

Top of the page