- Top
- Playback
- Thumbnail operations
- Reconnecting incomplete clips

# Reconnecting incomplete clips

Incomplete clips may be generated when clips recorded on multiple P2 cards (connected clips) are separately copied from each card. The reconnection function generates one clip (the original, connected clip) from incomplete clips.

Use the control stick to select incomplete clips to be linked.

Usually, thumbnails of incomplete clips (clips with indication) are displayed next to each other.

Select [RE-CONNECT] in the main menu → [CLIP] and press the control stick.

Select [YES] using the control stick.

This reconnects incomplete clips.

NOTE

- Incomplete clip indicators will remain displayed when only some clips are reconnected, unless all the constituent clips of the original clip are reconnected.

Top of the page