- Top
- Connecting to External Devices
- Connecting with headphones, remote control, or TV/monitor
- TV/monitor

# TV/monitor

A TV or monitor can be connected as shown in the following figure.

Audio cable (optional)

3.5 mm diameter jack-pin conversion cable

HDMI cable (optional)

BNC cable (optional)

BNC cable (optional)

TV/monitor

NOTE

- VIERA Link is not supported on the camera. Please be aware that when using an HDMI cable and connecting this camera to a device that supports VIERA Link, the VIERA Link of other devices may not work in some cases.

- SD signals (480i, 576i) output from the <HDMI OUT> terminal are converted to progressive signals (480P, 576P) then output.

- For the BNC cable (optional) connected to the <SDI OUT> terminal, prepare a double-shielded cable equivalent to 5C-FB.

- Prepare the HDMI cable (optional) with double shielded. For the HDMI cable, using Panasonic HDMI cable is recommended.

Top of the page