- Top
- Connecting to External Devices
- Linking to External Devices
- Connecting the video and monitor

# Connecting the video and monitor

The camera directly controls the video and the monitor to output video.

Audio pin cable*1

Video equipment/monitor

HDMI cable*2

BNC cable (composite/SDI)*3

Cables are optionally available. They are not supplied with the camera.

Prepare the HDMI cable (optional) with double or more shielded. For the HDMI cable, use of the Panasonic HDMI cable is recommended.

For the BNC cable (optional) connected to the <SDI OUT1>, <SDI OUT2>, and <VIDEO OUT> terminals, prepare a double-shielded cable equivalent to 5C-FB.

Top of the page