- Top
- Preparation
- Preparing for audio input
- Using the front microphone

# Using the front microphone

Microphones such as the stereo microphone kit AJ-MC900G (optional) can be mounted.

Viewfinder clamping screw

Viewfinder

Microphone holder

<MIC IN> terminal

Fig. 1

Fig. 2

Fig. 3

Open the microphone holder. (Fig. 1)

Mount the microphone and tighten the viewfinder clamping screw. (Fig. 2)

Mount with the UP indication on the microphone facing up.

Connect the microphone cable to the <MIC IN> terminal on the camera. (Fig. 3)

According to the audio channel to be recorded, switch the <AUDIO IN> switch to <FRONT>.

Top of the page