- Top
- Connecting to External Devices
- Connecting to the extension control unit (AG-EC4G)
- Switch functionality in remote control mode

# Switch functionality in remote control mode

The following switches and buttons on the camera do not function in remote control mode.

- <SHUTTER> switch

- <MENU> button

- Jog dial button

- <GAIN> selector switch

- <OUTPUT>/<AUTO KNEE> selector switch

- <WHITE BAL> switch

- <USER MAIN> button

- <USER 1> button

- <USER 2> button

Top of the page