- Top
- Connecting to External Devices
- Connecting to P2 ROP application

# Connecting to P2 ROP application

Using a P2 ROP application that operates on an iPad connected to the camera via wireless LAN, you can remotely control some functions of the camera.

For the settings for network connection, refer to “Setting for connection with P2 ROP application”.

For details on operation of the P2 ROP application, refer to the help file for P2 ROP application.

Switch functionality in remote control mode
Recording and playback operations in remote control mode

NOTE

- The status adjusted by connecting the P2 ROP application will always be recorded on the camera.

- When the camera is connected to the P2 ROP application, the P2 playlist editing function is not available.

Top of the page