- Top
- Menu Operations
- Setting menu structure
- Main menu structure

# Main menu structure

[PAINT] | These are items for performing fine image adjustments while monitoring the output waveform of the camera using the waveform monitor. You will need support from video engineers to use configure these settings. These menu item settings are enabled when using the camera as a standalone device. These menu items can be set from an external remote controller. These menu items cannot be set when the thumbnail screen is displayed.
[VF] | These items are shown when selecting contents to show in the viewfinder screen. These menu items cannot be set when the thumbnail screen is displayed.
[CAMERA] | These are items for changing the settings based on the condition of subject when the camera is operated. These menu items cannot be set when the thumbnail screen is displayed.
[CLIP] | These items are used when performing various tasks, such as playing back, deleting, and copying clips, and editing metadata, while checking the thumbnail of the clips displayed in the LCD monitor. These menu items are enabled when the thumbnail screen is displayed. Clip operations such as [DELETE] or [COPY] are enabled when the target thumbnail is selected. Some items are displayed only in specific situations such as in USB storage mode or on the explorer screen.
[REC/PB] | These are various types of setting items when performing camera recording and playback.
[I/F SETUP] | These are items for setting related to audio and video input/output and display, and setting battery, audio, video output, etc.
[FILE] | These are items for performing file-related operations such as reading from an SD memory card containing menu settings data, and handling lens files and lens chromatic aberration correction (CAC) files. These menu items cannot be set when the thumbnail screen is displayed or during playback.
[MAINTENANCE] | These are items for performing maintenance inspection of the camera. These menu items cannot be set when the thumbnail screen is displayed.
[SYSTEM] | These items are used for checking and updating the camera’s firmware version. Set the system frequency, the number of lines, and recording format.
[USER MENU SEL] | This menu is used to set the items to be displayed in [USER MENU]. For details on items that can be set, refer to “Setting items to [USER MENU] and loading/reading the settings to a data file”.

Top of the page