- Top
- Maintenance
- Warning system
- Warning/error displays in the thumbnail operation, menu operation, and USB storage mode

# Warning/error displays in the thumbnail operation, menu operation, and USB storage mode

#### Thumbnail and menu

Message | Description | Measure
--- | --- | ---
[AUTHENTICATION ERROR!] | Manual authentication failed. | Enter the correct password.
[CANNOT ACCESS!] | Data cannot be accessed due to a content defect or some other reason. | Ensure the health of the media and the clips.
[CANNOT CHANGE!] | For a clip with the mark, where a thumbnail cannot be generated, the thumbnail cannot be modified in the text memo position. | Correct the settings and content to enable display of the thumbnail.
[CANNOT DELETE!] | The content versions do not match. Cannot delete. | Match the device and contents version.
[CANNOT FORMAT!] | A P2 card problem or some other reason prevents formatting. | Check the P2 card.
[CANNOT RE-CONNECT!] | Clips cannot be remerged because either clips not recorded across multiple P2 cards are selected or other reasons. | Check the selected content.
[CANNOT REPAIR IN SELECTION!] | Some of the selected clips cannot be repaired. | Check the selected content.
[CANNOT REPAIR!] | Content that cannot be repaired is selected. | Check the selected content.
[CANNOT SAVE!][FILE NAME IN USE] | A settings file of the same name exists on the SD memory card. | Use another name to save the file.
[CARD FULL!] | The P2 card or SD memory card is full. | Insert a card with free space available.
[COPY IMPOSSIBLE. TOO LARGE CLIP CONTAINED!] [CLIP NAME:] (clip name) | Files exceeding 4 GB cannot be copied to a P2 memory card or microP2 memory card with 32 GB or lower capacity. | Copy to a microP2 memory card with capacity larger than 32 GB.
[INVALID VALUE!] | The data value you entered is invalid. | Enter data within the normal range.
[LACK OF CAPACITY!] | There is not enough recording capacity left on the card. | Insert a card with sufficient recording capacity.
[MISSING CLIP!] | Shot marks cannot be attached to the clips unless all clips recorded over multiple P2 cards are present. | Insert all P2 cards over which recording extended.
[NO CARD!] | No P2 or SD memory card is inserted. | Insert the relevant media.
[NO COPY TO SAME CARD!] | A clip cannot be copied to the card storing the original clip. | Copy the selected clip to a card that does not contain the original clip.
[NO FILE!] | The specified file does not exist. | Check the file.
[NO INPUT!] | No data is entered. | Enter data and then set.
[NO SD CARD!] | No SD memory card. | Insert an SD memory card.
[NOT SELECTED!] | Attempted to delete without selecting clips. | Select clips to delete.
[SAME CLIP IS SELECTED!] | Multiple instances of the same clip (copies) are included in the clips selected. | Multiple instances of the same clip (copies) cannot be copied simultaneously. Remove instances of the same clip from selected items.
[TOO MANY CLIPS!] | Too many clips are selected. | Reduce the number of selected clips.
[UNKNOWN CONTENTS FORMAT!] | This is a warning of the contents for the version that is not supported by the camera. | Match the device and content versions.
You cannot write back only proxy recording clips from the FTP server to the P2 card. | Write back (import) proxy recording clips to an SD memory card.
[UNKNOWN DATA!] | The metadata character code is invalid. | The metadata character code is UTF-8. Enter valid characters using a viewer.
There is a problem with data in the file. | Create the file again.
[USER CLIP NAME MODIFIED!] | When adding a counter value to the clip name, characters must be deleted. | For the counter addition setting, the user clip name plus the counter value can only contain up to 100 bytes. Characters in the clip name are automatically deleted when the total number of characters exceeds this limit.
[WRITE PROTECTED!] | The P2 card or SD memory card is write-protected. | Insert write-accessible media.
[CANNOT OPERATE THIS MENU, WHILE "REC DURING UPLOAD" ENABLED.] | The menu cannot be executed. | Set [DISABLE] in the main menu → [I/F SETUP] → [USB/LAN] → [FTP CLIENT SERVICE] → [REC DURING UPLOAD] before execution.

#### Soft keyboard

Message | Description | Measure
--- | --- | ---
[AUTHENTICATION ERROR!] | Manual authentication failed. | Enter the correct password.
[CANNOT CHANGE!] | An attempt is made to enter the [PERSON] item (user who enters the memo) when there is no text memo. | Enter the [TEXT] (text information) first.
[CANNOT SET!] [INVALID VALUE!] | The entered value is invalid. | Change the input value.
[CANNOT SET!] [NO INPUT!] | There is not input to the software keyboard. | Enter the password.
[CANNOT SET!] [RETRY PASSWORD IS DIFFERENT!] | The re-entered password is different. | Enter the correct reference password.

#### Storage

Message | Description | Measure
--- | --- | ---
[CANNOT ACCESS CARD!] | An error occurred while accessing the P2 card. | Check the P2 card.
[CANNOT ACCESS TARGET!] | An error occurred while accessing the connection target. | Check the storage device status and connection.
[CANNOT COPY!][FORMAT STORAGE DEVICE TO FAT] | The partition that can copy clips does not exist on the storage device. | Reformat in FAT format, or export the P2 card to create a partition.
[CANNOT FORMAT!] | The storage device cannot be formatted. | Change the connected storage device.
[CANNOT RECOGNIZE STORAGE DEVICE!] | The storage device is not correctly recognized. | Reboot the storage device or connect another storage device.
[CANNOT SELECT!][MAX. 6 PARTITIONS] | Storage devices with more than 6 partitions cannot be selected (mounted simultaneously). | Release selected partitions.
[CARD IS EMPTY! CANNOT COPY!] | The P2 card to copy is empty. | The copy operation is not performed because the card is empty.
[FORMAT P2 CARD!] | Cannot import to a P2 card containing clips. | Format the P2 card.
[LACK OF CAPACITY!] | Not enough space left on the storage device. | Use a new storage device with sufficient available space or a formatted storage device.
[MISMATCH COMPONENT!] | The P2 card model number of the copy source and copy destination do not match. Cannot copy. | Use the P2 cards of the same model number, or import on a clip basis.
[STORAGE DEVICE DISCONNECTED!] | The connection with the storage device is disconnected. | Reconnect the USB cable to the <USB3.0> terminal (host). When it does not function normally after that, turn off the power once and turn on the power again.
[TOO MANY PARTITIONS!] | There are too many partitions. | The maximum number of partitions on the storage device is 23. Either reformat, or use a new storage device.
[UNKNOWN DEVICE CONNECTED!] | A non-compatible DVD drive or other device is connected. | Change the connected device to the correct storage device, and then turn the power off once and turn it on again.
[VERIFICATION FAILED!] | The compare check performed after copying failed. | Copy it again.

Top of the page