- Top
- Shooting
- Viewfinder status display
- Waveform monitor function

# Waveform monitor function

A waveform of the video can be displayed by assigning the waveform monitor function to the <USER> buttons (<USER MAIN>/<USER1>/<USER2>) and pressing the assigned buttons. Press the button again to return to the normal display.

- The waveform and vector displays can be switched by [WFM] ([WFM]) in the main menu → [CAMERA] → [SW MODE]. Whether to display the waveform monitor on either or both of the viewfinder and LCD monitor can be selected by [WFM DISP].

- The waveform is not displayed while the focus assist function [EXPAND] is active.

- The waveform display cannot be recorded.

Top of the page