- Top
- Network Connection
- Using FTP client function
- Transferring from an SD memory card to an FTP server (export)

# Transferring from an SD memory card to an FTP server (export)

You can collectively transfer the data in an SD memory card to the FTP server.

Press the <THUMBNAIL> button.

The thumbnail screen is displayed.

Select [SD CARD] in the main menu → [CLIP] → [EXPORT].

Press the jog dial button (or the <SET> button).

The folders of FTP server are displayed.

Select the transfer destination folder using the jog dial button (or the cursor buttons (/)).

Press the <SET> button while pressing the <SHIFT> button (<MULTI SEL>) to create a new folder in the current folder list. Numbers that indicate date and time are automatically entered as the name of the new folder. You can also use the software keyboard to set the folder name. However, some characters cannot be used depending on the FTP server. You cannot set a folder name that is same as an existing folder.

Move the cursor to [YES] and press the <SET> button.

Exporting starts.

When exporting is completed, [COPY COMPLETED!] appears.

NOTE

- You cannot select clips to be exported.

- Folder names using multi-byte characters are not displayed correctly.

- Depending on factors such as the number of files, file sizes, and network conditions, exporting may take time.

- To discontinue the export process, press the <SET> button. On the [CANCEL] confirmation message that appears, select [YES] and press the <SET> button. If the network has not been disconnected, the partially exported files remaining on the FTP server are deleted. If the network has been disconnected, incomplete files may remain on the FTP server.

- After exporting starts, disconnection errors will no longer be detected. Cancel the export operation if the copying progress has stalled.

- Contact your FTP server administrator for the amount of free space on the FTP server in advance, as it cannot be checked automatically before exporting starts.

- Whether an error is generated when the remaining capacity of the FTP server reaches 0 depends on the FTP server. If an error is not generated, cancel the export operation.

- If existing folders are selected and files that have the same path names as data in the SD memory card are included in the selected folders, the files are overwritten. However, if the path names are the same but the types differ (folder and file), an error is generated.

- To prevent unintended overwriting, create new folders to export data whenever possible.

- To transfer clips using SSH, the FTP server must support SSH.

- Using SSH will reduce the transfer speed.

Top of the page