- Top
- Maintenance
- Troubleshooting
- For operations

For operations

Problem | Cause/solution
The camera cannot be turned on. | Does the power cable plugged into the power outlet securely?
The camera cannot be operated from the ROP (AK-HRP1000G) that is connected via IP. | Is the power turned on? If the power lamp of the camera is not lit, the power of the camera is off.
Is a valid IP address of the camera set?
Is the correct camera to be operated selected?
Is the camera connected with the ROP (AK-HRP1000G) correctly? Also refer to the Operating Instructions of AK-HRP1000G.
The ROP (AK-HRP1000G) may require upgrading to support the camera. Contact your dealer.

Top of the page