- Top
- Menu Operations
- Menu list
- [SYSTEM MODE]

# [SYSTEM MODE]

[FORMAT] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[FORMAT] | Sets the system format. [1080/59.94p], [1080/50p], [1080/29.97p], [1080/25p], [1080/23.98p], [1080/59.94p-240fps], [1080/50p-200fps] Factory setting: [1080/59.94p]
[HDR SW] | — | Enables/disables the HDR mode. [OFF], [ON] Factory setting: [OFF]
[COLORIMETRY] | Switches the coefficient for the Y/C conversion. [BT.709], [BT.2020] Factory setting: [BT.709] NOTE When [HDR SW] is set to [OFF], the setting is disabled and will be set to [BT.709].
[SHOOTING MODE] | Sets the shooting mode. [NORMAL], [HIGH SENS] Factory setting: [NORMAL]
[CABLE CONNECTION] | Set the connection method used between the camera and CCU. [HYBRID], [FIBER] Factory setting: [HYBRID]

Top of the page