- Top
- Menu Operations
- Menu list
- [FILE]

# [FILE]

## [SD CARD]

[SD CARD] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[MODE] | Selects the operation mode. [FORMAT], [LOAD], [STORE] Factory setting: [LOAD]
[FILE SEL] | Selects a file. [ALL], [ALL SCENE], [ALL USER], [ALL LENS], [SCENE], [USER], [LENS] Factory setting: [SCENE]
[FILE NO.] | Selects a file number. [CURRENT], [1]…[8] (Scene file) [1]…[3] (User file) [1]…[32] (Lens file) [CURRENT] (Operation file) Factory setting: [1]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [SCENE1]
[SD FILE NO.] | Selects the file number of the SD memory card. [1]…[100] Factory setting: [1]
[EXECUTE] | Selects whether to execute with the configured settings. [NO], [YES]

## [SCENE FILE]

Item | Description of settings
--- | ---
[MODE] | Selects the operation mode. [LOAD], [STORE] Factory setting: [LOAD]
[FILE NO.] | Selects a file. When [MODE] is set to [LOAD]: [OFF], [1]…[8] Factory setting: [OFF] When [MODE] is set to [STORE]: [1]…[8] Factory setting: [1]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [SCENE1]
[EXECUTE] | Selects whether to execute with the configured settings. [NO], [YES]

## [USER FILE]

Item | Description of settings
--- | ---
[MODE] | Selects the operation mode. [LOAD], [STORE] Factory setting: [LOAD]
[FILE NO.] | Selects a file. [1], [2], [3] Factory setting: [1]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [USER1]
[EXECUTE] | Selects whether to execute with the configured settings. [NO], [YES]

## [REFERENCE FILE]

Item | Description of settings
--- | ---
[MODE] | Selects the operation mode. [LOAD], [STORE] Factory setting: [LOAD]
[FILE NO.] | Selects a file. [1], [2], [3] Factory setting: [1]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [REFERENCE1]
[EXECUTE] | Selects whether to execute with the configured settings. [NO], [YES]

## [CAC FILE]

[CAC FILE] cannot be selected right after the power is turned on, because boot of the camera is in progress.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[CARD FILE SELECT] | Selects a file. [1]…[100] Factory setting: [1]
[READ] | Loads CAC files. [YES], [NO]
[DELETE] | Deletes the CAC file in the SD memory card. [NO], [YES]

Top of the page