- Top
- Web Screen
- [Setup] screen
- [Basic] screen

# [Basic] screen

Item | Description of settings
--- | ---
[Camera title] | Enter the name of the camera. Clicking the [Set] button displays the entered name on the camera title display area. The factory setting value is the product number of the camera. You can enter 0 to 20 single-byte characters. Characters that can be used Single-byte numbers: 0123456789 Single-byte alphabet (upper/lower case): ABCDEFGHIJKLMNOPQRSTUVWXYZ abcdefghijklmnopqrstuvwxyz Single-byte symbols: !#$%'()*+,-./:;<=>?@[]^_`{|}~\
[Automatic installation of viewer software] | Configures automatic installation of the plugin software for display. [On]: Installs the plugin software for display automatically. [Off]: Does not install the plugin software for display automatically. Factory setting: [On]
[Smoother live video display on the browser (buffering)] | Configures settings for display of images on the camera using the plugin software for display. [On]: Stores images on the camera to the computer temporarily to make images to be displayed smoother. [Off]: Does not store images on the camera to the computer and displays images in real time. Image display and audio playback are not available on a computer where the plugin software for display Network Camera View 4S is not installed. The number of times that the plugin software for display has been installed can be viewed in the [Product info.] tab of the [Maintenance] menu in the [Setup] screen. Factory setting: [On]

Top of the page