- Top
- Menu Operations
- Menu list
- [MAINTENANCE]

# [MAINTENANCE]

## [LENS FILE ADJUST]

Item | Description of settings
--- | ---
[LENS FILE SW] | Switches the enable/disable of the lens file. [OFF], [ON] Factory setting: [OFF]
[LENS FILE MODE] | Selects the operation mode. [LOAD], [STORE], [CANCEL] Factory setting: [LOAD]
[FILE NO.] | Selects a file. [1] - [32] Factory setting: [1]
[FILE NAME] | Enters a file name. (15 characters or less) Factory setting: [LENS FILE 1]
[EXECUTE] | Selects whether to execute. [NO], [YES]
[FLARE R] | Adjusts Rch flare of the data selected in [FILE NO.]. [−100] - [+100] Factory setting: [0]
[FLARE G] | Adjusts Gch flare of the data selected in [FILE NO.]. [−100] - [+100] Factory setting: [0]
[FLARE B] | Adjusts Bch flare of the data selected in [FILE NO.]. [−100] - [+100] Factory setting: [0]
[GAIN R] | Adjusts Rch gain of the data selected in [FILE NO.]. [−100] - [+100] Factory setting: [0]
[GAIN B] | Adjusts Bch gain of the data selected in [FILE NO.]. [−100] - [+100] Factory setting: [0]
[W H SAW R] | Adjusts Rch white shading for the data selected in [FILE NO.] horizontally using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[W H SAW G] | Adjusts Gch white shading for the data selected in [FILE NO.] horizontally using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[W H SAW B] | Adjusts Bch white shading for the data selected in [FILE NO.] horizontally using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[W H PARA R] | Adjusts Rch white shading for the data selected in [FILE NO.] horizontally using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[W H PARA G] | Adjusts Gch white shading for the data selected in [FILE NO.] horizontally using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[W H PARA B] | Adjusts Bch white shading for the data selected in [FILE NO.] horizontally using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[W V SAW R] | Adjusts Rch white shading for the data selected in [FILE NO.] vertically using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[W V SAW G] | Adjusts Gch white shading for the data selected in [FILE NO.] vertically using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[W V SAW B] | Adjusts Bch white shading for the data selected in [FILE NO.] vertically using a saw-toothed waveform. [−100] - [+100] Factory setting: [0]
[W V PARA R] | Adjusts Rch white shading for the data selected in [FILE NO.] vertically using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[W V PARA G] | Adjusts Gch white shading for the data selected in [FILE NO.] vertically using a parabolic waveform. [−100] - [+100] Factory setting: [0]
[W V PARA B] | Adjusts Bch white shading for the data selected in [FILE NO.] vertically using a parabolic waveform. [−100] - [+100] Factory setting: [0]

## [BLACK SHADING]

Item | Description of settings
--- | ---
[CORRECT] | Enables/disables the auto correction function of black shading. [OFF], [ON] Factory setting: [ON]
[DETECTION] | Selects whether to execute auto correction function of black shading. [NO], [YES]
[SAVE] | Selects whether to save the auto correction data. [NO], [YES]
[CLEAR] | Selects whether to clear the auto correction data. [NO], [YES]

## [FAN SETTING]

Item | Description of settings
--- | ---
[FAN MODE] | Sets the operation mode of the air cooling fan. [AUTO], [LOW] Factory setting: [AUTO] NOTE Use in an environment with ambient temperature of 30 °C (86 °F) or less when using in [LOW].

## [INITIALIZE]

[READ FACTORY ALL DATA] cannot be selected right after the power is turned ON, or when 59.94, 29.97, 23.98 and 50, 25 in [FORMAT] are switched since the unit is starting up.

This is not an error. Perform operation after a while.

Item | Description of settings
--- | ---
[MENU INITIALIZE] | Restores the value of [MAIN MENU] to their factory settings. [YES], [NO]
[READ USER ALL DATA] | Restores the values of [MAIN MENU], scene file and user file to their factory settings. [YES], [NO]
[READ FACTORY ALL DATA] | Restores the values of [MAIN MENU], scene file, user file, and the factory adjusted values to their factory settings. [YES], [NO]

Top of the page