- Top
- UB300 Setting Tool
- Operation
- Connection setting screen

# Connection setting screen

This is the screen displayed when the [Connection Setting] button is clicked. This is also displayed during startup.

1. [Camera]

   - [IP Address]

     Sets the IP address of AK-UB300G to be connected.

   - [Port]

     Sets the port number of AK-UB300G to be connected.

     This setting is not necessary when the HTTP port number at the AK-UB300G side is not changed from its default.

2. [Authentication]

   - [User Name]

     Specifies the account name used to connect to AK-UB300G. Specify the account with the administrator privilege.

   - [Password]

     Specifies the password for the account to be used when connecting.

3. [Local Host]

   - [Port]

     Specifies the communication port number of the personal computer where the UB300 Setting Tool is to operate.

4. [Connect] button

   Connection to AK-UB300G will start when the [Connect] button is clicked after setting [IP Address]/[Port]/[User Name]/[Password].

   [AK-UB300] is displayed in [Model] when the connection is successful.

Top of the page