- Top
- Connecting to External Devices
- Connecting the remote operation panel (AK-HRP1000G/AK-HRP1005G)

# Connecting the remote operation panel (AK-HRP1000G/AK-HRP1005G)

- Some of the functions can be controlled remotely by connecting the remote operation panel AK-HRP1000G/AK-HRP1005G (optional).

NOTE

- Update the version of the remote operation panel as described below.

  AK-HRP1000G: 4.21-00-0.00 or later

  AK-HRP1005G: 4.21-00-0.00 or later

- For details, refer to the operating instructions of the remote operation panel and supplied flyer.

Serial connection with the <I/F> terminal
IP connection with the <LAN> terminal
Top of the page