- Top
- Maintenance
- Warning displays
- Other warning displays

# Other warning displays

Together with the displaying the content of the warning, the <WARNING> lamp will illuminate in red, and the front tally lamp and the back tally lamp will blink in red.

[FAN NG] | There is a problem in the fan.
[HIGH TEMPERATURE] | The internal temperature is high.
[LOW VOLTAGE] | The voltage of the external DC power supply is low.
[SHUTDOWN SOON] | The internal temperature is rising more than expected. Or, the voltage of the external DC power supply has lowered beyond the operation guarantee. The power is turned off forcefully in 30 seconds.

Top of the page