- Top
- Menu Operations
- Menu list
- [DISPLAY SETUP]

# [DISPLAY SETUP]

## [MARKER]

Item | Description of settings
--- | ---
[FOCUS ASSIST SW] | Enables/disables the focus assist switch. [OFF], [ON] Factory setting: [OFF]
[FOCUS ASSIST] | — | Displays the type of the focus assist.
| [IN RED SW] | Enables/disables the IN RED switch. [OFF], [ON] Factory setting: [OFF]
| [IN RED COLOR] | Sets the color for IN RED. [RED], [GREEN] Factory setting: [RED]
| [BAR SW] | Enables/disables the BAR switch. [OFF], [ON] Factory setting: [OFF]
| [MAG SW] | Enables/disables the magnification display function. [OFF], [ON] Factory setting: [OFF]
[ZEBRA] | — | Enables/disables the luminance zebra. [OFF], [ON] Factory setting: [OFF]
| [ZEBRA1 LEVEL] | Sets the level of the luminance zebra 1. [0%] - [109%] Factory setting: [80%]
| [ZEBRA2 LEVEL] | Sets the level of the luminance zebra 2. [0%] - [109%] Factory setting: [100%]
| [ZEBRA PATTERN] | Sets the pattern of the luminance zebra. [1], [1+2], [SPOT] Factory setting: [1]
[FRAME LEVEL SWITCH] | — | Shows/hides the level display outside the frame marker. [OFF], [ON] Factory setting: [OFF]
| [FRAME LEVEL] | Sets the level to be displayed outside the frame marker. [0] - [15] Factory setting: [15]
[FRAME MARK SWITCH] | Shows/hides the frame marker. [OFF], [ON] Factory setting: [OFF]
[FRAME SIG] | Sets the aspect ratio of the frame marker. [4:3], [13:9], [14:9], [15:9], [16:9], [CINEMA], [VISTA] Factory setting: [4:3]
[SAFETY MARK SWITCH] | Shows/hides the safety marker. [OFF], [ON] Factory setting: [OFF]
[SAFETY MARK] | Sets the aspect ratio of the safety marker. [16:9], [15:9], [14:9], [13:9], [4:3] Factory setting: [16:9]
[SAFETY AREA] | Sets the size of the safety area. [80%] - [100%] Factory setting: [80%]
[CENTER MARK] | — | Shows/hides the center marker. [OFF], [ON] Factory setting: [OFF]
| [CENTER MARK SELECT] | Sets the size of the center marker. [1] - [7] Factory setting: [1]
[MARKER LEVEL] | Sets the brightness of the markers and on-screen display. [50%], [60%], [70%], [80%], [90%], [100%] Factory setting: [100%]

## [MONITOR DISPLAY]

Item | Description of settings
--- | ---
[F NUMBER] | Shows/hides the iris display (F value). [OFF], [ON] Factory setting: [OFF] This is displayed when you use a lens that outputs position information.
[ZOOM] | Shows/hides the zoom position display. [OFF], [ON] Factory setting: [OFF] This is displayed when you use a lens that outputs position information.
[EXTENDER] | Shows/hides the extender display. [OFF], [ON] Factory setting: [OFF]
[FILTER] | Shows/hides the filter position display. [OFF], [ON] Factory setting: [OFF]
[MASTER GAIN] | Shows/hides the master gain display. [OFF], [ON] Factory setting: [OFF]
[SHUTTER] | Shows/hides the electronic shutter display. [OFF], [ON] Factory setting: [OFF]
[DIGITAL EXTENDER] | Shows/hides the digital extender display. [OFF], [ON] Factory setting: [OFF]
[DRS] | Shows/hides the dynamic range stretcher display. [OFF], [ON] Factory setting: [OFF]
[STATUS(AUTO)] | Shows/hides the display appearing when AWB/ABB are activated or deactivated. [OFF], [ON] Factory setting: [OFF]
[SYSTEM MODE] | Shows/hides the system frequency/resolution display. [OFF], [ON] Factory setting: [OFF]
[COLOR TEMP] | Shows/hides the color temperature display. [OFF], [ON] Factory setting: [OFF]
[FBC] | Shows/hides the flash band compensation display. [OFF], [ON] Factory setting: [OFF]
[SHOOTING MODE] | Shows/hides the sensitivity mode display. [OFF], [ON] Factory setting: [OFF]
[MAG] | Shows/hides the focus assist expanded display. [OFF], [ON] Factory setting: [ON]
[TALLY] | Shows/hides the tally display. [OFF], [ON] Factory setting: [OFF]
[FRAME MIX] | Shows/hides the frame mix (total gain) display. [OFF], [ON] Factory setting: [OFF]
[AGC] | Shows/hides the auto gain control display. [OFF], [ON] Factory setting: [OFF]
[ATW] | Shows/hides the auto tracking white balance display. [OFF], [ON] Factory setting: [OFF]
[HAZE REDUCTION] | Shows/hides the haze elimination mode display. [OFF], [ON] Factory setting: [OFF]

Top of the page