- Top
- Specifications
- Specifications
- General

# General

Power DC 12 V (DC 11 V–17 V) Power consumption 40 W (body only, when 3G SDI×4 is output) 60 W (maximum power when all accessories are connected and each output terminal is outputting at maximum)

indicates safety information.

Ambient operating temperature | −10 °C – 45 °C (14 °F – 113 °F) (Preheating required under a temperature 0 °C (32 °F) or below)
Storage temperature | −20 °C – 60 °C (−4 °F – 140 °F)
Ambient operating humidity | 85% or less (relative humidity)
Weight | Approx. 1.6 kg (3.53 lbs.) (body only)
Dimensions (W×H×D) | Body only 110 mm×140 mm×160 mm (4-11/32 inches×5-17/32 inches×6-5/16 inches) (excluding protrusions)

Top of the page