- Top
- Operation
- Multi-formats

# Multi-formats

The video output method for UHD, HD crop (UHD CROP) from UHD and HD can be selected with [MAIN MENU] → [SYSTEM MODE] → [FORMAT].

- The output from the <HD SDI OUT 1> terminal and the <UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals are used for the main line.

- The output from the <HD SDI OUT 2> terminal is used for the monitor.

Superimposing of character
List of output formats (<UHD/HD SDI OUT 1> to <UHD/HD SDI OUT 4> terminals)
List of output formats (<HD SDI OUT 1>/<HD SDI OUT 2> terminals)
Top of the page