- Top
- Operation
- Image quality adjustment
- White clip function

# White clip function

This function sets the brightest part of video signals to be not brighter than a certain level.

#### General settings

Use the camera with the factory settings.

#### Advanced settings

Sets in [MAIN MENU] → [PAINT] → [WHITE CLIP].

[WHITE CLIP]: Selects [ON]/[OFF] of the white clip function. The [MASTER WHITE CLIP LEVEL] setting value is enabled when set to [ON].

[MASTER WHITE CLIP LEVEL]: Sets the white clip level.

[R WHITE CLIP LEVEL]: Sets the clip level of Rch for white clips.

[B WHITE CLIP LEVEL]: Sets the clip level of Bch for white clips.

Top of the page