- Top
- Operation
- Image quality adjustment
- Knee function

# Knee function

This function sets the compression of video signals to prevent halation in images.

#### General settings

Use the camera with the factory settings.

#### Advanced settings

Set in [MAIN MENU] → [PAINT] → [KNEE].

- When [AUTO] is selected in [MAIN MENU] → [PAINT] → [KNEE] → [KNEE]

  [AUTO KNEE RESPONSE]: Sets the speed of response. The smaller the setting value, the faster the response speed.

- When [MANUAL] is selected in [MAIN MENU] → [PAINT] → [KNEE] → [KNEE]

  [KNEE MASTER POINT]: Sets the knee point position in 0.25% steps.

  [KNEE MASTER SLOPE]: Sets the knee inclination.

  [KNEE R SLOPE]: Sets the knee inclination of Rch.

  [KNEE B SLOPE]: Sets the knee inclination of Bch.

Top of the page