- Top
- Operation
- Image quality adjustment
- RB gain control function

# RB gain control function

This is a function to set to add or reduce intensity of red and blue.

This operates with automatic white balance. This will not operate with auto tracking white balance.

#### General settings

Use the camera with the factory settings.

#### Advanced settings

Set in [MAIN MENU] → [PAINT] → [RB GAIN CONTROL SETTING].

- When [RB GAIN PRESET] is selected

  [R GAIN]: Sets to add or reduce intensity in red.

  [B GAIN]: Sets to add or reduce intensity in blue.

- When [RB GAIN] is selected

  [R GAIN]: Sets to add or reduce intensity in red.

  [B GAIN]: Sets to add or reduce intensity in blue.

  [GAIN OFFSET]: Sets whether to maintain the value set in [R GAIN] and [B GAIN], or to reset when the automatic white balance is performed.

Top of the page