- Top
- Operation
- Image quality adjustment
- Detail function

# Detail function

This function thickens or weakens the outlines of images. It effectively softens or sharpens images, but in some cases, the whole image may become coarse due to emphasized noise and edges.

To avoid such phenomenon, it is necessary not to add this effect on parts where emphasizing is not needed and keep the details of the parts.

#### General settings

[MASTER DETAIL]: Sets the level of the detail effect of the whole part.

[CRISP]: Sets the level of signal (including noise) not to activate the detail effect.

#### Advanced settings

Set this in [MAIN MENU] → [PAINT] → [DETAIL SETTING].

[DETAIL]: Sets [ON]/[OFF] of the detail function.

[V DETAIL LEVEL]: Sets the intensity of the detail level in the vertical direction.

[PEAK FREQUENCY]: Sets the thickness of detail in the horizontal direction.

[V DETAIL FREQUENCY]: Sets the thickness of detail in the vertical direction.

[LEVEL DEPENDENT]: Detail in the darker area is compressed when the detail of luminosity signal is emphasized. Detail of bright area is also compressed more when the value set for [LEVEL DEPENDENT] is larger.

[KNEE APERTURE LEVEL]: Sets the detail level of high luminosity areas (high-brightness areas).

[DETAIL GAIN(+)]: Sets the detail level toward the + direction (making brighter).

[DETAIL GAIN(−)]: Sets the detail level toward the − direction (making darker).

Top of the page