- Top
- Web Screen
- [Setup] screen
- [Basic] screen

# [Basic] screen

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
Camera title |  | Input the name of the camera here. When the [Set] button is clicked, the input name appears in the camera title display area. The factory default setting is the model number of the unit. You can enter between 0 to 20 half-size characters. Characters that can be used Half-size numeric characters: 0123456789 Half-size alphabetical characters (upper and lower cases): ABCDEFGHIJKLMNOPQRSTUVWXYZ abcdefghijklmnopqrstuvwxyz Symbols: !#$%'()*+,-./:;<=>?@[]^_`{|}~\
Automatic installation of viewer software | On Off | One of the following settings is selected for the automatic installation of the plug-in viewer software. On The plug-in viewer software is automatically installed. Off The plug-in viewer software is not automatically installed.
Smoother live video display on the browser (buffering) | On Off | Configure settings for displaying images from the unit on the plug-in viewer software. On Temporarily store images from the unit onto the personal computer for smoother display. Off Do not temporarily store images from the unit onto the personal computer, and display them in real time. Images and audio cannot be viewed or listened to on personal computers on which the “Network Camera View 4S” plug-in viewer software is not installed. You can view the number of times the plug-in software was installed under the [Product info.] tab in the [Maintenance] menu of the unit’s [Setup] screen.

Top of the page