- Top
- Reference
- Connector pin assignment table
- Front panel

# Front panel

#### [INTERCOM] connector

HA16PRH-5S (Hirose Electric Co., Ltd.)

Pin No. | Function | Remarks
--- | --- | ---
1 | SHIELD | Carbon MIC: -1 dB Dynamic MIC: -5 dB Select [DYN] , [ECM], or [CBN] in [MIC TYPE] that can be accessed by selecting [CCU INTERCOM TALK] in the [AUDIO] menu.
2 | TALK
3 | SHIELD
4 | RECEIVE
5 | NC

Top of the page