- Top
- Picture monitor (PM)
- Transition of displays

# Transition of displays

When trouble is detected, warning information is automatically displayed on the picture monitor.

Even if status information or operation information is already displayed on the picture monitor when trouble is detected, priority is given to the display of the warning information.

The descending sequence of priority for the displays on the picture monitor is as follows: warning displays → auto displays → status displays → ROP menu displays → CCU menu displays → operation displays → no display.

When the warning information with the highest priority disappears, the warning information with the next highest priority appears.

Priority | Screen | ROP connected
--- | --- | ---
Yes | No
High ↑ ↓ Low | Warning displays | Warnings are automatically displayed when trouble is detected. Self-recovery The warning displays are cleared Press the [CHARA] button of the ROP No display→(WARNING)→ IRIS →Status displays→ Status1 → Status2 → Status3 → Status4 → Status5 → Status6 → Status7 → IRIS ・・・ Hold down the [CHARA] button of the ROP The warning displays are cleared | Warnings are automatically displayed when trouble is detected. Self-recovery The warning displays are cleared Press the [USER1] button of this unit (This is enabled when [CHARA] is assigned to the button.) When the transition source screen is displayed: The display switches to the transition source screen. When the transition source screen is not displayed: The warning displays are cleared
Auto displays | Automatically displayed | Automatically displayed
Status displays | Perform display operations using the [CHARA] button of the ROP. Press the [CHARA] button of the ROP No display→(WARNING)→ IRIS →Status displays→ Status1 → Status2 → Status3 → Status4 → Status5 → Status6 → Status7 → IRIS ・・・ Hold down the [CHARA] button of the ROP The status displays end. | –
CCU menu displays When the camera menu is displayed from the ROP while a menu of the CCU (this unit) is displayed, the menu of the CCU (this unit) disappears. | Display by pressing the menu button on the unit. Operations using the [SELECT] dial on the unit | Display by pressing the menu button on the unit. Operations using the [SELECT] dial on the unit
Operation displays | Automatically displayed | Automatically displayed
No display | – | –

Top of the page