- Top
- CCU menu
- MAINTENANCE
- SD CARD

# SD CARD

This is the selection screen for the SD CARD menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
DATA SAVE | - | Save the unit's setting information to memory card. When you select this, the execution confirmation screen (NO?, YES?) appears.
DATA LOAD | - | Load the unit's setting information saved in memory card to this unit. When you select this, the execution confirmation screen (NO?, YES?) appears.
LOG FILE DOWNLOAD | - | Save CCU (this unit) log information to memory card. When you select this, the execution confirmation screen (NO?, YES?) appears.
UPDATE | - | Upgrade the unit's software or programs (FPGA) with files saved to the memory card. When you select this, the execution confirmation screen (NO?, YES?) appears.
CARD FORMAT | - | Initialize the memory card. When you select this, the execution confirmation screen (NO?, YES?) appears. Initialization may take about 5 minutes. Be sure to execute initialization after confirming the data because any data that is deleted by the initialization cannot be recovered.

#### Data Stored/Loaded

The following data is stored/loaded.

- Items in the [OPERATION] menu

- Items in the [MAINTENANCE] menu

(The [NETWORK] menu, [VERSION] menu, [SYSTEM] menu, and [SD CARD] menu are excluded.)

- Items in the [SYSTEM] menu

#### SD Card Error Messages

When an error occurs during processing of SD card menu items, the following messages are displayed.

Messages | Content and remedy
--- | ---
LOAD ERROR | Unable to read from the memory card. Data written with other than this unit cannot be read.
WRITE ERROR | Unable to write to the memory card. The memory card is likely to be defective. Replace the memory card.

Top of the page