- Top
- CCU menu
- AUDIO
- MIC OUT

# MIC OUT

This is the selection screen for the MIC OUT menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
MIC1 OUT GAIN | 0dB +4dB | This switches the analog output gain for MIC1.
MIC1 OUT LV | -40dB to 0dB to +20dB | This adjusts the analog output level for MIC1.
MIC2 OUT GAIN | 0dB +4dB | This switches the analog output gain for MIC2.
MIC2 OUT LV | -40dB to 0dB to +20dB | This adjusts the analog output level for MIC2.

Top of the page