- Top
- CCU menu
- Basic menu operations
- Text input

# Text input

1.Turn the [SELECT] dial to move the cursor to the menu item where text is to be input, and then press the [SELECT] dial.

The cursor display changes as indicated by "↓". By turning the [SELECT] dial, you can move the cursor to the next (previous) character position.

2.Turn the [SELECT] dial to move the cursor to position where a character is to be input, and then press the [SELECT] dial.

The selected character starts flashing and you can change it.

3.Turn the [SELECT] dial to change the character, and then press the [SELECT] dial.

Turning the [SELECT] dial changes characters, and pressing the [SELECT] dial confirms character changes.

When a character has been input and the flashing stops, you can move the cursor.

If you press the [SELECT] dial while the cursor is on the left of a menu item, the cursor becomes “→” and you can select the menu item.

NOTE

- Turning the [SELECT] dial clockwise while pressing it increases the speed at which the number increases (turning it counterclockwise decreases the number). Turning the dial more increases the speed even more. This operation is effective for making a large change to a value when the setting width is large (e.g., IP address or port number).

Top of the page