- Top
- CCU menu
- MAINTENANCE
- PM VIEW SETTING(1/2)

# PM VIEW SETTING(1/2)

This is the selection screen for the PM VIEW SETTING(1/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
CAMERA NO | ON OFF | Set display of the camera number on the picture monitor to ON or OFF.
SYSTEM FORMAT | ON OFF | Set display of the system format on the picture monitor to ON or OFF.
FORMAT MODE | ON OFF | Set display of the format mode on the picture monitor to ON or OFF.
SCENE FILE No | ON OFF | Set display of the scene file number on the picture monitor to ON or OFF.
SHUTTER | ON OFF | Set display of the shutter value on the picture monitor to ON or OFF.
ND/CC FILTER | ON OFF | Set display of the ND/CC filter name to the picture monitor to ON or OFF.
EXTENDER INFO | ON OFF | Set display of extender information (extender and digital extender) on the picture monitor to ON or OFF.
IRIS | ON OFF | Set display of the IRIS F value on the picture monitor to ON or OFF.
IRIS LEVEL | ON OFF | Set display of the IRIS level bar on the picture monitor to ON or OFF. When [OFF] is set, the IRIS menu is not displayed on the picture monitor.
IRIS SCALE | FULL 2STOP | Set the IRIS display range of the status display screen.
COLOR TEMP VALUE | ON OFF | Set display of the color temperature on the picture monitor to ON or OFF.
IRIS MEMORY | ON OFF | Set display of the IRIS value stored in camera memory on the picture monitor to ON or OFF.

Top of the page