- Top
- Web Screen (AK-NP600)
- Displaying the web screen (AK-NP600)
- Displaying the web screen using a personal computer

# Displaying the web screen using a personal computer

Screens from Windows (Microsoft Edge) are used as examples in this manual. There will be some differences in how the screen appears in other browsers, but the procedures will be the same.

1.Start the web browser of the personal computer.

Use one of the web browsers below depending on the operating system installed in the personal computer.

Installed OS | Web browser
--- | ---
Windows | Microsoft Edge Internet Explorer 11 Google Chrome
macOS | Safari

2.Enter the IP address you configured on the EasyIP Setup Tool Plus in the address bar of the web browser.

Example of input

http://registered URL

http://192.168.0.52

If this unit is within a local network, make the settings for the proxy server from the web browser so that the proxy server is not used for the local address.

3.Sets the initial account.

If the web screen is set to be shown in the initial state, the initial account setting screen is displayed.

Set the user name and password.

NOTE

- Do not use a string of characters that can be easily guessed by a third party.

- Change your password regularly.

- Use at least 3 of the following 4 character types in a password of at least 8-characters in length.

Upper case alphabet

Lower case alphabet

Numbers

Symbols (! # $ % ’ ( ) * + , - . / ? @ [ ] ^ _ ` ~)

- If a password is set that does not follow the above policy, the user assumes responsibility for operation, with an adequate understanding of the security risks to the installation environment, etc.

- A warning message is displayed if you set a password that does not meet the recommended setting policy. To change the password, click the [Back] button and enter another password.
  To continue the settings after understanding the risk to security, click [Continue] and then complete the settings.

- If you have forgotten the account information you set, execute [SYSTEM] > [FACTORY INITIALIZE] in the CCU menu, and reset the user information used for network connections.
  The settings for this unit return to the factory settings when you execute [FACTORY INITIALIZE].

“Initialize the Unit Settings (INITIALIZE)”

4.Complete registration of the initial account.

The following screen indicating registration completion is displayed after registration of the initial account is complete.

After about 10 seconds of showing this completion screen, the settings screen is automatically shown. If the screen does not transition to the settings screen even after 10 seconds have elapsed, click on the link in “please click here” to move to the settings screen manually.

This completes the procedures for registering the initial account

5.Display the settings screen.

The web screen is displayed.

In the initial screen, the Product information screen [Product info.] is displayed, so switch if necessary.

Top of the page