- Top
- CCU menu
- MAINTENANCE
- NETWORK(2/2)

# NETWORK(2/2)

This is the selection screen for the NETWORK(2/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
IP TALLY | INDEX NO | 1 to 254 (Factory setting: 1) | Sets the INDEX NO set by devices that output TALLY.
PORT | 60000 to 65535 (Factory setting: 62000) | Sets the PORT number for TALLY IN.
SET EXECUTE | - | When you press the [SELECT] button, [NETWORK(2/2) SET EXECUTE NO/YES] appears. Select [YES] to apply the configured [NETWORK(2/2)] information to the unit. If this operation is not performed, the changed [NETWORK(2/2)] settings will not be applied. In addition, if you exit the menu without performing this operation, the settings will return to their original values.

Top of the page