- Top
- CCU menu
- MAINTENANCE
- PM VIEW SETTING(2/2)

# PM VIEW SETTING(2/2)

This is the selection screen for the PM VIEW SETTING(2/2) menu.

___ indicates factory default settings.

Item | Setting value | Setting details
--- | --- | ---
TALLY INFO | ON OFF | Set display of the tally information on the picture monitor to ON or OFF.
F.DROP | ON OFF | Shows/hides the F.DROP that is notified by the camera, on the picture monitor.
ZOOM POSITION | ON OFF | Set display of the zoom position information, which is notified by the camera, on the picture monitor to ON or OFF.
FOCUS POSITION | ON OFF | Set display of the focus position information, which is notified by the camera, on the picture monitor to ON or OFF.
OPT_CAM | ON OFF | Set display of the optical signal level (camera side) on the picture monitor to ON or OFF.
OPT_CCU | ON OFF | Set display of the optical signal level (CCU side) on the picture monitor to ON or OFF.
COLORIMETRY | ON OFF | Set display of COLORIMETRY (Y/C conversion coefficient), which is notified by the camera, on the picture monitor to ON or OFF.
V-LOG | ON OFF | Shows/hides V-LOG information.

Top of the page