- Top
- Operation
- Menu setting contents
- [FILE] menu

# [FILE] menu

Saves and reads the setting data.

For saving and loading target, refer to “Target items for scene file/setup file/initialization”.

For details of saving and loading, refer to “Handling setting data”.

## [SCENE FILE]

[LOAD] | Selects the scene file saved in the SD card and reads it into the camera. Can select if all of the scene files ([SCENE1] to [SCENE5]) are read, or individually read.
[SAVE] | The setting value of the current scene file ([SCENE1] to [SCENE5]) is overwritten to the file selected from the list of scene files saved in the SD card.
[SAVE AS] | The setting value of the current scene file ([SCENE1] to [SCENE5]) is saved to the SD card as a new scene file by entering the file name.

## [SETUP FILE]

[LOAD] | Selects the setup file saved in the SD card and reads it into the camera.
[SAVE] | Overwrites the file selected in the list of the setup files saved in the SD memory card with the current setting value of the camera.
[SAVE AS] | Saves the current setting value in the camera as a new setup file in the SD card by entering the file name.

## [SLOT FOR SCENE/SETUP FILE]

Sets the card slot to read and save the scene file and the setup file.

The items that can be set are as follows.

- [SLOT1], [SLOT2]

(Factory setting: [SLOT1])

Top of the page